SELF-TROUBLESHOOTING GUIDE

Workflow which involves open CV, Image Processing embedded in raspberry pi to chat with the user( Telegram) to have the step wise instructions for self-troubleshooting their Appliances

Includes Features like

1. all kinds of barcode detection
2. Enabling chat with Telegram Application
3. Image( circle) detection (Image Processing )
4. Sending the data from pi to a Local host
5. Displaying the web page in Local host